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Safety Data Sheet MSDS
三氧化二铁
Ferric Oxide 
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：三氧化二铁Product Chinese name: Ferric Oxide
产品英文名称：Ferric Oxide
Product English name:  Ferric Oxide
CAS No.：1309-37-1
型号Model：DXN-FE50,DXN-FE200.
分子式：Fe2O3
Molecular formula: Fe2O3
分子量：159.69
Molecular weight: 159.69
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	三氧化二铁
Ferric Oxide
	99%
	用作磁性材料、颜料、擦光剂、催化剂等，也用于油漆、油墨和塑料的着色。
Used as magnetic materials, pigments, polishes, catalysts, etc., and also used for coloring paints, inks and plastics.




3.危险性概述
Hazards Identification

危险类别（GHS）：非危险物质或混合物。
Hazard Class (GHS): Not a hazardous substance or mixture.
健康危害：可刺激呼吸道，引起皮肤刺激和眼睛刺激。
Health hazards: May cause respiratory irritation, skin irritation and eye irritation.

4.急救措施
First aid measures
 
皮肤接触：用大量肥皂水和水清洗。脱去受污染的衣服和鞋子，脱下被污染的衣物前请用水彻底冲洗，或者戴手套。连续冲洗至少十分钟。寻求医疗救护。
Skin contact: Wash with plenty of soap and water. Remove contaminated clothing and shoes, rinse thoroughly with water before removing contaminated clothing, or wear gloves. Continue to rinse for at least ten minutes. Seek medical attention.
眼睛接触：立即用大量水冲洗眼睛，并不时提起上下眼睑。检查和取出任何隐形眼镜。连续冲洗至少十分钟。寻求医疗救护。
Eye contact: Immediately flush eyes with plenty of water, occasionally lifting the upper and lower eyelids. Check and remove any contact lenses. Continue flushing for at least ten minutes. Get medical attention.
吸入：将患者转移到空气新鲜处，休息，保持利于呼吸的体位。如沒有呼吸，呼吸不规则或呼吸停止，由受过训练的人员进行人工呼吸或给氧。寻求医疗救护。
Inhalation: Move the patient to fresh air, rest, and maintain a position conducive to breathing. If not breathing, breathing irregularly or breathing has stopped, have trained personnel perform artificial respiration or give oxygen. Seek medical attention.
食入：用水冲洗口腔，有假牙请摘掉。若物质已被吞下且患者保持清醒，可饮少量水， 患者感到恶心就应停止，因为呕吐会有危险。禁止催吐，除非有专业医疗人士指导，发生呕吐，应保持头部朝下以避免呕吐物进入肺部。寻求医疗救护。切勿给失去意识者任何口服物。
Ingestion: Rinse mouth with water and remove dentures if present. If material has been swallowed and the person is conscious, give small amounts of water to drink. Stop if the person feels nauseous because vomiting can be dangerous. Do not induce vomiting unless directed by a medical professional. If vomiting occurs, keep the head down to prevent vomitus from entering the lungs. Seek medical attention. Never give anything by mouth to an unconscious person.

5.消防措施
Fire-fighting measures

灭火方法及灭火剂：用水雾,耐醇泡沫,干粉或二氧化碳灭火。
Fire extinguishing methods and extinguishing agents: Extinguish with water spray, alcohol-resistant foam, dry powder or carbon dioxide.  

6.泄露应急处理
Leakage emergency treatment

人员的预防,防护设备和紧急处理程序：使用个人防护设备。防止粉尘的生成。防止吸入蒸汽、气雾或气体。保证充分的通风，将人员撤离到安全区域。 
Personal precautions, protective equipment and emergency procedures: Use personal protective equipment. Prevent dust generation. Prevent inhalation of vapors, mists or gases. Ensure adequate ventilation and evacuate personnel to safe areas.
环境预防措施:避免溢出物扩散和流走，避免溢出物接触进入土壤、河流、下水道和污水管道。如产品已经导致环境污染（下水道，水道，土壤或空气），请通知有关当局。
Environmental precautions: Avoid spills from spreading and running away, and avoid spills from coming into contact with soil, rivers, drains and sewage pipes. If the product has caused environmental pollution (drains, waterways, soil or air), please inform the relevant authorities.
抑制和清除溢出物的方法和材料: 将容器移离泄漏区域。 用吸尘器清理或彻底清扫污染物并将其放在贴有指定标签的废弃物容器中。 
Methods and materials for containment and cleanup: Move containers away from spill area. Vacuum or sweep up contamination and place in a designated, labeled waste container.

7.操作处置和储存
Handling and storage

安全操作的注意事项: 防止粉尘和气溶胶生成。在有粉尘生成的地方,提供合适的排风设备。一般性的防火保护措施。
Precautions for safe handling: Prevent dust and aerosol formation. Provide suitable exhaust ventilation where dust is generated. General fire protection measures.安全储存的条件,包括任何不兼容性:按照当地法规要求来储存。储存于原装容器中，防止直接光照，置于干燥、凉爽和通风良好的区域，远离禁忌物、食品和饮料，上锁保管。使用容器前，保持容器关紧与密封。已开封的容器必须小心地再封好，并保持直立以防止漏出。请勿储存在未加标签的容器中。采用合适的收容方式以防止污染环境。 
Conditions for safe storage, including any incompatibilities: Store in accordance with local regulations. Store in original container, protected from direct sunlight, in a dry, cool and well-ventilated area, away from incompatible materials, food and beverages, and locked up. Keep container tightly closed and sealed until use. Opened containers must be carefully resealed and kept upright to prevent leakage. Do not store in unlabeled containers. Use appropriate containment to prevent environmental contamination.

8.接触控制和个体防护
Exposure controls and personal protection

工程控制：尽可能安装封闭体系或局部排风系统，操作人员切勿直接接触。同时安装淋浴器和洗眼器。
Engineering control:Install a closed system or local exhaust system as much as possible, and operators should not come into direct contact with it. Also install a shower and eyewash station.
呼吸系统防护：作业工人建议佩戴防尘口罩。
Respiratory system protection: Workers are recommended to wear dust masks.
眼睛防护：戴化学安全防护眼镜。
Eye protection: Wear chemical safety glasses.
身体防护：防护服。
Body protection: Protective clothing. 
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：及时换洗工作服。注意个人清洁卫生。
Other protection: Change and wash work clothes in time. Pay attention to personal hygiene.

9.理化特性
Physical and chemical properties

	颜色Color
	红棕色Reddish brown

	状态State
	粉末Powder

	气味Odor
	无味Odorless

	溶解度
Solubility
	不溶于水，在浓酸中加热逐渐溶解
Insoluble in water, gradually dissolves when heated in concentrated acid

	相对密度
Relative density
	5.120

	熔点Melting point
	1538℃



10.稳定性和反应性
Stability and reactivity

稳定性：本产品在标准大气状态(室温)下化学性质稳定。
Stability: The chemical properties of this product are stable under standard atmospheric conditions (room temperature).
[bookmark: _GoBack]不相容的材料：氯甲酸酯, 过氧化物, 强酸强酸, 过氧化物, 氯甲酸酯。
Incompatible Materials: Chloroformates, Peroxides, Strong AcidsStrong Acids, Peroxides, Chloroformates.

11.毒理学资料
Toxicology Information

急性毒性：无资料
Acute toxicity: No data

12.生态学资料
Ecological information

无资料No data

13.废弃处置
Waste disposal

废弃处置方法：应尽可能避免或减少废物的产生。产品、溶液和其副产品的处置应符合环境保护、废弃物处理法规和当地相关法规的要求。经由特许的废弃物处理合同商处理剩余物与非再生产品。废物不应未经处置就排入下水道，除非完全符合所有管辖权内主管机构的要求。包装废弃物应回收，仅在回收利用不可行时，才考虑焚烧或填埋。采用安全的方法处理本品及其容器。操作处置没有清洁或冲洗的空容器时，应小心处理。空的容器或内衬可能保留一些产品的残余物。避免溢出物扩散和流走，避免溢出物接触进入土壤、河流、下水道和污水管道。
Waste disposal method: The generation of waste should be avoided or reduced as far as possible. The disposal of products, solutions and their by-products should comply with the requirements of environmental protection, waste disposal regulations and relevant local regulations. Dispose of surplus and non-recycled products through licensed waste disposal contractors. Waste should not be discharged into the sewer without treatment unless the requirements of the competent authorities in all jurisdictions are fully met. Packaging waste should be recycled, and only when recycling is not feasible, incineration or landfill should be considered. Use safe methods to dispose of this product and its container. When handling empty containers without cleaning or rinsing, they should be handled with care. Empty containers or liners may retain some product residues. Avoid the spread and runoff of spills and avoid spills from contacting soil, rivers, sewers and sewage pipes.

14.运输信息
Transport information

运输品名：三氧化二铁
Transport name: Ferric Oxide
危险品分类：普货。
Dangerous goods classification: General goods.
运输注意事项：储存于阴凉、通风仓间内，保持容器密封。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。操作现场不得吸烟、饮水、进食。
Transport precautions: Store in a cool, ventilated warehouse and keep the container sealed. Be careful when handling to prevent damage to the packaging and container. Pay attention to personal protection during packaging and handling. Do not smoke, drink water, or eat at the operation site.

15.法规信息
Regulatory Information

适用法规：中华人民共和国安全生产法;
中华人民共和国职业病防治法;
中华人民共和国环境保护法;
危险化学品安全管理条例;
安全生产许可证条例。
Applicable regulations: Production Safety Law of the People's Republic of China;
Occupational Disease Prevention and Control Law of the People's Republic of China;
Environmental Protection Law of the People's Republic of China;
Regulations on the Safety Management of Hazardous Chemicals;
Regulations on Production Safety Permits.

16. 其他信息
Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
Modification instructions：Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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