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Safety Data Sheet MSDS
氢氧化铝
Aluminium Hydroxide
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：氢氧化铝Product Chinese name: Aluminium Hydroxide
产品英文名称：Aluminium Hydroxide
Product English name: Aluminium Hydroxide
CAS No.：21645-51-2 
型号Model：DXN-QYAL200.
分子式：H3AlO3
Molecular formula: H3AlO3
分子量：78.00
Molecular weight: 78.00
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	氢氧化铝
Aluminium Hydroxide
	30%
	阻燃剂、抛光剂、催化剂载体、陶瓷釉料等
Flame retardants, polishing agents, catalyst carriers, ceramic glazes, etc.

	水
Water
	70%
	




3.危险性概述
Hazards Identification

危险类别（GHS）：非危险物质或混合物。
Hazard Class (GHS): Not a hazardous substance or mixture.

4.急救措施
First aid measures
 
[bookmark: _GoBack]皮肤接触：用肥皂清洗及用清水洗至少 15 分钟，迅速就医治疗已红肿及生水泡之皮肤。
Skin contact: Wash with soap and water for at least 15 minutes, and seek medical attention immediately for any redness, swelling, or blisters.
眼睛接触：立即用大量的清水至少持续冲洗 15 分钟，送眼科医生诊疗。
Eye contact: Immediately rinse with plenty of water for at least 15 minutes and seek medical attention from an ophthalmologist.
吸入：将人移至空气新鲜处以提供所需氧气。
Inhalation: Move the person to fresh air to provide necessary oxygen.
食入：不可送入任何东西给没知觉或痉挛病人口中，应让有知觉或清醒的病人饮大量的水。不可催 吐，迅速就医治疗。
Ingestion: Do not put anything into the mouth of an unconscious or convulsing patient. Conscious or conscious patients should be allowed to drink plenty of water. Do not induce vomiting and seek medical treatment immediately.

5.消防措施
Fire-fighting measures

灭火方法及灭火剂：用水雾,抗乙醇泡沫,干粉或二氧化碳灭火。
Fire extinguishing methods and extinguishing agents: Use water spray, alcohol-resistant foam, dry powder or carbon dioxide to extinguish fire.

6.泄露应急处理
Leakage emergency treatment

人员的预防,防护设备和紧急处理程序：防止粉尘的生成。 防止吸入蒸汽、气雾或气体。
Personal precautions, protective equipment and emergency procedures: Prevent dust formation. Prevent inhalation of vapors, mists or gases.
环境预防措施:不要让产物进入下水道。
Environmental precautions: Do not allow product to enter drains.
抑制和清除溢出物的方法和材料:扫掉和铲掉。 存放在合适的封闭的处理容器内。
Methods and materials for containment and cleanup: Sweep up and shovel. Store in suitable closed disposal containers.

7.操作处置和储存
Handling and storage

安全操作的注意事项:在有粉尘生成的地方,提供合适的排风设备。
Precautions for safe handling: Provide suitable exhaust equipment where dust is generated.
安全储存的条件,包括任何不兼容性:贮存在阴凉处.容器保持紧闭，储存在干燥通风处。存放于惰性气体环境中。远离不相容的材料比如氧化剂存放。
Conditions for safe storage, including any incompatibilities: Store in a cool place. Keep the container tightly closed in a dry and ventilated place.Store in an inert gas environment. Keep away from incompatible materials such as oxidants.

8.接触控制和个体防护
Exposure controls and personal protection

工程控制：密闭操作，局部排风
Engineering control:Closed operation, local exhaust ventilation.
呼吸系统防护：作业工人建议佩戴防尘口罩。
Respiratory system protection: Workers are recommended to wear dust masks.
眼睛防护：戴化学安全防护眼镜。
Eye protection: Wear chemical safety glasses.
身体防护：防护服。
Body protection: Protective clothing. 
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：及时换洗工作服。注意个人清洁卫生。
Other protection: Change and wash work clothes in time. Pay attention to personal hygiene.

9.理化特性
Physical and chemical properties

	颜色Color
	白色White

	状态State
	粉末Powder

	气味Odor
	无味Odorless

	溶解度
Solubility
	不溶于水和醇，能溶于无机酸和碱溶液Insoluble in water and alcohol, soluble in inorganic acid and alkali solutions

	相对密度
Relative density
	2.42g/cm3

	熔点Melting point
	300℃



10.稳定性和反应性
Stability and reactivity

稳定性：一般情况下稳定。
Stability: Generally stable.
特殊情况：将氢气化铝加热至 200℃以上，会有水蒸汽急速释出。此时须驱散水蒸汽及降低其产生之压力，急速增 加的压力会导致设备受损甚至爆炸。
Special case: When aluminum hydride is heated to above 200℃, water vapor will be released rapidly. At this time, the water vapor must be dispersed and the pressure generated must be reduced. Rapidly increasing pressure may cause damage to the equipment or even explosion.
禁配物: 强酸
Incompatible materials: Strong acids.
 
11.毒理学资料
Toxicology Information

急性毒性：：LD50 经口 - 大鼠 - 雌性 - > 2,000 mg/kg
Acute toxicity: LD50 Oral - Rat - Female - > 2,000 mg/kg

12.生态学资料
Ecological information

生态毒性：无数据资料
Ecotoxicity: No data available

13.废弃处置
Waste disposal

废弃处置方法：产品废弃物：假如无法重复使用或是回收，可丢弃于垃圾掩埋处理场。包装材料废弃物：建议根据当地或政府的法定规定丢弃。
Waste disposal method: Product waste: If it cannot be reused or recycled, it can be disposed of in a landfill.Packaging material waste: It is recommended to dispose of it according to local or government regulations.

14.运输信息
Transport information

运输品名：氢氧化铝
Transport name: Aluminium Hydroxide
危险品分类：普货
Dangerous goods classification: General goods.
运输注意事项：储存于阴凉、通风仓间内。远离火种、热源。保持容器密封，应与氧化剂、食用化 工原料分开存放。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。
Transport precautions: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. Keep the container sealed and store it separately from oxidants and edible chemical raw materials. Load and unload gently during transportation to prevent damage to the packaging and container. Pay attention to personal protection during packaging and transportation.

15.法规信息
Regulatory Information

适用法规：职业安全卫生法
事业废弃物贮存清除处理方法及设施标准
Applicable regulations: Occupational Safety and Health Law
Methods and facility standards for storage, removal and treatment of industrial waste

16. 其他信息
Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
Modification instructions：Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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