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Safety Data Sheet MSDS
氢氧化镍
Nickel Hydroxide
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：氢氧化镍Product Chinese name: Nickel Hydroxide
产品英文名称：Nickel Hydroxide
Product English name: Nickel Hydroxide
CAS No.：12054-48-7
型号Model：DXN-NI200.
分子式：H2NiO2
Molecular formula: H2NiO2
分子量：92.73
Molecular weight: 92.73
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	氢氧化镍
Nickel Hydroxide
	99%
	纺织品，陶瓷，塑料，纤维，涂料，消毒液等
Textiles, ceramics, plastics, fibers, coatings, disinfectants, etc




3.危险性概述
Hazards Identification

危险类别（GHS）：非危险物质或混合物。
Hazard Class (GHS): Not a hazardous substance or mixture.

4.急救措施
First aid measures
 
皮肤接触：用肥皂水及清水彻底冲洗。就医。若有灼伤，按碱灼伤处理。
Skin contact: Rinse thoroughly with soap and water. Seek medical attention. If burns occur, treat as alkaline burns.
眼睛接触：拉开眼睑，用流动清水冲洗15分钟。就医。
Eye contact: Pull open the eyelids and rinse with running water for 15 minutes. Seek medical attention.
吸入：脱离现场至空气新鲜处。呼吸困难时给输氧。呼吸停止时，立即进行人工呼吸。就医。
Inhalation: Leave the scene and go to fresh air. Give oxygen if breathing is difficult. If breathing stops, perform artificial respiration immediately. Seek medical attention.
食入：误服者，口服牛奶、豆浆或蛋清，就医。
Ingestion: If ingested by mistake, take milk, soy milk or egg white orally and seek medical attention.

5.消防措施
Fire-fighting measures

灭火方法及灭火剂：用水雾、干粉、泡沫或二氧化碳灭火剂灭火。
Fire extinguishing methods and extinguishing agents: Use water spray, dry powder, foam or carbon dioxide to extinguish fire.

6.泄露应急处理
Leakage emergency treatment

人员的预防,防护设备和紧急处理程序：建议应急处理人员戴携气式呼吸器，穿防静电服，戴橡胶耐油手套。禁止接触或跨越泄漏物。作业时使用的所有设备应地.尽可能切断泄漏源。消除所有点源。根据液体流动、蒸汽或粉尘扩散的影响区域划定警戒区，无关人员从侧风、上风向撤离至安全区。
Personal precautions, protective equipment and emergency procedures: It is recommended that emergency response personnel wear air-carrying respirators, anti-static clothing, and rubber oil-resistant gloves. It is prohibited to touch or cross the leaked material. All equipment used during the operation should be grounded. Cut off the source of leakage as much as possible. Eliminate all point sources. Delineate warning areas according to the affected areas of liquid flow, steam or dust diffusion, and irrelevant personnel evacuate to safe areas from the sidewind and upwind directions.
环境预防措施:收容泄漏物，避免污染环境。防止泄漏物进入下水道、地表水和地下水。
Environmental precautions: Contain the leak to avoid environmental contamination. Prevent the leak from entering sewers, surface water and groundwater.
抑制和清除溢出物的方法和材料:小心扫起，避免扬尘，运至废物处理场所。用水刷洗泄漏污染区，经稀释的污水放入废水系统。如大量泄漏，收集回收或无害处理后废弃。
Methods and materials for containment and cleanup: Sweep it up carefully to avoid raising dust, and transport it to a waste disposal site. Wash the leaked area with water, and put the diluted sewage into the wastewater system. If there is a large amount of leakage, collect it for recycling or dispose of it harmlessly.

7.操作处置和储存
Handling and storage

安全操作的注意事项:在有粉尘生成的地方,提供合适的排风设备。
Precautions for safe handling: Provide suitable exhaust equipment where dust is generated.
安全储存的条件,包括任何不兼容性:储存于阴凉、通风仓间内。保持容器密封。应与氧化剂、酸类分开存放。操作现场不得吸烟、饮水、进食。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。
Conditions for safe storage, including any incompatibilities: Store in a cool, ventilated warehouse. Keep the container sealed. Store away from oxidants and acids. Do not smoke, drink or eat at the operation site. Load and unload gently during transportation to prevent damage to the packaging and container. Pay attention to personal protection during subpackaging and transportation.

8.接触控制和个体防护
Exposure controls and personal protection

工程控制：密闭操作，局部排风
Engineering control:Closed operation, local exhaust ventilation.
呼吸系统防护：作业工人建议佩戴防尘口罩。
Respiratory system protection: Workers are recommended to wear dust masks.
眼睛防护：戴化学安全防护眼镜。
Eye protection: Wear chemical safety glasses.
身体防护：防护服。
Body protection: Protective clothing. 
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：及时换洗工作服。注意个人清洁卫生。
Other protection: Change and wash work clothes in time. Pay attention to personal hygiene.

9.理化特性
Physical and chemical properties

	颜色Color
	绿色Green

	状态State
	粉末Powder

	气味Odor
	无味Odorless

	溶解度
Solubility
	微溶于水，溶于酸、氨水。
Slightly soluble in water, soluble in acid and ammonia.

	相对密度
Relative density
	4.15

	熔点Melting point
	230℃



10.稳定性和反应性
Stability and reactivity

稳定性：一般情况下稳定。
Stability: Generally stable.
禁配物:  强酸,强氧化剂。
Incompatible materials: Strong acid, strong oxidizing agent.
避免接触的条件：静电放电、热、潮湿等。
Conditions to avoid: static discharge, heat, moisture, etc.
 
11.毒理学资料
Toxicology Information

急性毒性：无数据资料
Acute toxicity: No data available

12.生态学资料
Ecological information

生态毒性：无数据资料
Ecotoxicity: No data available

13.废弃处置
Waste disposal

废弃处置方法：尽可能回收利用。如果不能回收利用，采用焚烧方法进行处置。不得采用排放到下水道的方式废 弃处置本品。
Waste disposal method: Recycle as much as possible. If recycling is not possible, dispose of it by incineration. Do not dispose of this product by discharge into the sewer.

14.运输信息
Transport information

运输品名：氢氧化镍
Transport name: Nickel Hydroxide
危险品分类：普货。
Dangerous goods classification: General goods.
运输注意事项：储存于阴凉、通风仓间内。远离火种、热源。保持容器密封，应与氧化剂、食用化 工原料分开存放。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。
Transport precautions: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. Keep the container sealed and store it separately from oxidants and edible chemical raw materials. Load and unload gently during transportation to prevent damage to the packaging and container. Pay attention to personal protection during packaging and transportation.

15.法规信息
Regulatory Information

适用法规：职业安全卫生法;
道路交通安全规则;
劳工作业场所容许暴露标准;
事业废弃物贮存清除处理方法及设施标准。
Applicable regulations: Occupational Safety and Health Law;
Road Traffic Safety Regulations;
Labor workplace exposure standards;
Industrial waste storage, removal and treatment methods and facility standards.

16. 其他信息
Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
[bookmark: _GoBack]Modification instructions：Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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