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Safety Data Sheet MSDS
氧化铜
Cupric Oxide
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：氧化铜
Product Chinese name: Cupric Oxide
产品英文名称：Cupric Oxide
Product English name:  Cupric Oxide
CAS No.：1317-38-0 
型号Model：DXN-KF40
分子式：CuO
Molecular formula: CuO
分子量：79.55
Molecular weight: 79.55
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	氧化铜
Cupric Oxide
	40%
	制人造丝、陶瓷、釉及搪瓷、电池、石油脱硫剂、杀虫剂Textiles, Manufacture of rayon, ceramics, glazes and enamels, batteries, petroleum desulfurizers, pesticides

	水
Water
	60%
	




3.危险性概述
Hazards Identification

危险类别（GHS）：非危险物质或混合物。
Hazard Class (GHS): Not a hazardous substance or mixture.
环境危害：有害
Environmental hazards: Harmful
燃爆危险：有毒，具有刺激性
Explosion hazards: Toxic, irritating

4.急救措施
First aid measures
 
皮肤接触：用肥皂水及清水彻底冲洗。就医。
Skin contact: Rinse thoroughly with soap and water. Seek medical attention.
眼睛接触：拉开眼睑，用流动清水冲洗15分钟。就医。
Eye contact: Pull open the eyelids and rinse with running water for 15 minutes. Seek medical attention.
吸入：脱离现场至空气新鲜处。就医。
Inhalation: Leave the scene to a place with fresh air. Seek medical attention.
食入：立即让伤者饮水（最多2杯）。 请教医生。
Ingestion: Give the injured person a drink of water immediately (up to 2 cups). Ask a doctor.

5.消防措施
Fire-fighting measures

灭火方法及灭火剂：用水雾,抗乙醇泡沫,干粉或二氧化碳灭火。
Fire extinguishing methods and extinguishing agents: Use water spray, alcohol-resistant foam, dry powder or carbon dioxide to extinguish fire.
灭火时可能遭遇之特殊危害：不可燃。周围火源可能引发释放危害性蒸气。
Special hazards that may be encountered during fire fighting: Non-flammable. Surrounding fire sources may cause the release of hazardous vapors.

6.泄露应急处理
Leakage emergency treatment

人员的预防,防护设备和紧急处理程序：防止粉尘的生成。 防止吸入蒸汽、气雾或气体。避免物质接触.，确保有充足的通风。撤出危险区域，遵照急救措施，请教专业人员。
Personal precautions, protective equipment and emergency procedures: Prevent dust formation. Prevent inhalation of vapors, mists or gases.Avoid contact with the substance. Ensure adequate ventilation. Evacuate the danger area, follow first aid measures, consult qualified personnel.
环境预防措施:不要让产物进入下水道。
Environmental precautions: Do not allow product to enter drains.
抑制和清除溢出物的方法和材料: 暗渠。收集，吸取与排出溅液遵照可能的物质使用限制干燥取出，丢弃，清理受影响的区域，避免灰尘生成。
Methods and materials for containment and cleanup: Collect, absorb and discharge spills following possible restrictions on use of materials. Remove dry, discard and clean the affected area, avoiding dust generation.

7.操作处置和储存
Handling and storage

安全操作的注意事项:在有粉尘生成的地方,提供合适的排风设备。
Precautions for safe handling: Provide suitable exhaust equipment where dust is generated.
安全储存的条件,包括任何不兼容性:贮存在阴凉处.容器保持紧闭，储存在干燥通风处。存放于惰性气体环境中。远离不相容的材料比如氧化剂存放。
Conditions for safe storage, including any incompatibilities: Store in a cool place. Keep the container tightly closed in a dry and ventilated place.Store in an inert gas environment. Keep away from incompatible materials such as oxidants.

8.接触控制和个体防护
Exposure controls and personal protection

工程控制：密闭操作，局部排风
Engineering control:Closed operation, local exhaust ventilation.
呼吸系统防护：作业工人建议佩戴防尘口罩。
Respiratory system protection: Workers are recommended to wear dust masks.
眼睛防护：戴化学安全防护眼镜。
Eye protection: Wear chemical safety glasses.
身体防护：防护服。
Body protection: Protective clothing. 
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：及时换洗工作服。注意个人清洁卫生。
Other protection: Change and wash work clothes in time. Pay attention to personal hygiene.

9.理化特性
Physical and chemical properties

	颜色Color
	黑色Black

	状态State
	液体Liquid

	气味Odor
	无味Odorless

	相对密度
Relative density
	6.4g/cm3

	熔点Melting point
	1326℃



10.稳定性和反应性
Stability and reactivity

稳定性：一般情况下稳定。
Stability: Generally stable.
禁配物: 还原剂, 硫化氢气体, 铝, 碱金属, 金属粉末
Incompatible materials: Reducing agent, Hydrogen sulfide gas, Aluminum, Alkali metal, Metal powder
 
11.毒理学资料
Toxicology Information

急性毒性：LD50 大鼠: 470 mg/kg
Acute toxicity: LD50 rat: 470 mg/kg

12.生态学资料
Ecological information

生态毒性：对鱼类的毒性:LC50 Oncorhynchus mykiss（红鳟）: 25 mg/l; 96 h
Ecotoxicity: Toxicity to fish:LC50 Oncorhynchus mykiss (rainbow trout): 25 mg/l; 96 h
对水蚤和其他水生无脊椎动物的毒性：EC50 Daphnia magna（水蚤）: 0.04 mg/l; 48 h
Toxicity to daphnia and other aquatic invertebrates:EC50 Daphnia magna (water flea): 0.04 mg/l; 48 h

13.废弃处置
Waste disposal

废弃处置方法：废料的排放必须符合国家及当地法规的规范。废弃化学品请保留于原容器中，勿与其他废弃物混合。依照处理产品的相同标准处理不洁的容器。
Waste disposal method: Waste discharge must comply with national and local regulations. Keep waste chemicals in their original containers and do not mix with other waste. Dispose of dirty containers in the same manner as products..

14.运输信息
Transport information

运输品名：氧化铜
Transport name: Cupric Oxide
危险品分类：普货。
Dangerous goods classification: General goods.
运输注意事项：起运时包装要完整，装载应稳妥。运输过程中要确保容器不泄漏、不倒場、不坠落、不损坏。严禁与还原剂、碱金属、食用化学品等混装混运。运输途中应防晒、雨淋，防高温。车辆运输完毕应进行彻店清扫。
Transport precautions: When shipping, the packaging should be complete and the loading should be secure. During transportation, make sure that the container does not leak, fall, fall, or be damaged. It is strictly prohibited to mix and transport with reducing agents, alkali metals, food chemicals, etc. During transportation, it should be protected from sun, rain and high temperature. After the vehicle is transported, the entire store should be cleaned.

15.法规信息
Regulatory Information

适用法规：中华人民共和国安全生产法;
中华人民共和国职业病防治法;
中华人民共和国环境保护法;
危险化学品安全管理条例;
安全生产许可证条例。
Applicable regulations: Production Safety Law of the People's Republic of China;
Occupational Disease Prevention and Control Law of the People's Republic of China;
Environmental Protection Law of the People's Republic of China;
Regulations on the Safety Management of Hazardous Chemicals;
Regulations on Production Safety Permits.

16. 其他信息
[bookmark: _GoBack]Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
Modification instructions：Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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