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Safety Data Sheet MSDS
氧化铬
Chromium oxide
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：氧化铬Product Chinese name: Chromium oxide
产品英文名称：Chromium oxide
Product English name: Chromium oxide
CAS No.：1308-38-9
型号Model：DXN-GR30.
分子式：Cr2O3
Molecular formula: Cr2O3
分子量：151.99
Molecular weight: 151.99
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	氧化铬
Chromium oxide
	30%
	用于陶瓷和搪瓷的着色，也可用作分析试剂，催化剂
Used for coloring ceramics and enamels, and can also be used as analytical reagents and catalysts

	水
Water
	70%
	




3.危险性概述
Hazards Identification

危险类别（GHS）：非危险物质或混合物。
Hazard Class (GHS): Not a hazardous substance or mixture.

4.急救措施
First aid measures
 
皮肤接触：脱去污染的衣着，用肥皂水和清水彻底冲洗皮肤。如有不适感。就医
Skin contact: Remove contaminated clothing and wash skin thoroughly with soap and water. If you feel any discomfort. Seek medical advice.
眼睛接触：提起眼睑，用流动清水或生理盐水冲洗。如有不适感，就医。
Eye contact: Lift your eyelids and rinse with running water or saline. If you feel unwell, seek medical attention.
吸入：迅速脱离现场至空气新鲜处，保持呼吸道通畅。如呼吸困难，输氧。
Inhalation: Leave the scene quickly to fresh air and keep your respiratory tract open. If breathing is difficult, give oxygen.
食入：饮足量温水，催吐。
Ingestion: Drink enough warm water to induce vomiting.

5.消防措施
Fire-fighting measures

灭火方法及灭火剂：本品不燃。根据着火原因选择合适灭火剂灭火。消防人员穿全身防火防毒服，在上风向灭火，尽可能将容器从火场移至空旷处。喷水保持火场容器冷却，直至灭火结束。切勿将水流直接射至熔融物，以免引起严重的流淌火灾。
Fire extinguishing methods and extinguishing agents: This product is non-flammable. Choose the appropriate fire extinguishing agent according to the cause of the fire. Firefighters should wear full-body fire-proof and gas-proof suits, fight fires in the upwind direction, and move containers from the fire scene to open areas as much as possible. Spray water to keep the fire container cool until the fire is extinguished. Never direct water flow into molten material to avoid serious flow fires.

6.泄露应急处理
Leakage emergency treatment

人员的预防,防护设备和紧急处理程序：隔离泄漏污染区，限制出入。建议应急处理人员戴防尘口罩。穿上适当的防护服前严禁接触破裂的容器和泄漏物。尽可能切断泄漏源。
Personal precautions, protective equipment and emergency procedures: Isolate the leaked contaminated area and restrict access. It is recommended that emergency responders wear dust masks. Do not touch ruptured containers and spilled materials before wearing appropriate protective clothing. Cut off the source of the leak as much as possible.
环境预防措施:不要让产物进入下水道。
Environmental precautions: Do not allow product to enter drains.
抑制和清除溢出物的方法和材料:用洁净的铲子收集泄漏物，置于干净、干燥、盖子较松的容器中，将容器移离泄漏区。
Methods and materials for containment and cleanup: Use a clean shovel to collect the leakage, place it in a clean, dry container with a loose lid, and move the container away from the leakage area.

7.操作处置和储存
Handling and storage

操作注意事项:密闭操作，加强通风。操作人员需经过专门培训，严格遵守操作规程。建议操作人员带防尘口罩，化学安全防护眼镜，穿一般工作服，戴橡胶手套。工作场所严禁抽烟。避免产生粉尘。
Operation precautions: Close operation and enhance ventilation. Operators need to receive special training and strictly abide by operating procedures. It is recommended that operators wear dust masks, chemical safety glasses, general work clothes, and rubber gloves. Smoking is strictly prohibited in the workplace. Avoid dust generation.
储存注意事项：储存于阴凉干燥，通风良好的库房。包装必须密封，切勿受潮，应与不相容材料、强酸强碱、食用化学品分开存放。切忌混储。
Storage precautions: Store in a cool, dry, well-ventilated warehouse. The packaging must be sealed and protected from moisture, and should be stored separately from incompatible materials, strong acids and alkalis, and edible chemicals. Avoid mixed storage.
8.接触控制和个体防护
Exposure controls and personal protection

工程控制：生产过程密闭操作，加强通风。
Engineering control:The production process is operated in a closed manner and ventilation is enhanced.
呼吸系统防护：可能接触其粉尘时，应该佩戴防尘口罩。必要时佩戴空气呼吸器。
Respiratory system protection: You should wear a dust mask when you may come into contact with its dust. Wear air respirator if necessary.
眼睛防护：戴防护眼镜。
Eye protection: Wear protective glasses.
身体防护：穿防护服。
Body protection: Wear protective clothing.
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：工作完毕，淋浴更衣，保持良好卫生习惯。
Other protection: After work, shower and change clothes, and maintain good hygiene habits.

9.理化特性
Physical and chemical properties

	颜色Color
	绿色Green

	状态State
	[bookmark: _GoBack]液体Liquid

	气味Odor
	无味Odorless

	溶解度
Solubility
	不溶于水、酸和碱溶液
Insoluble in water, acid and alkali solutions

	相对密度
Relative density
	5.21g/cm3

	熔点Melting point
	2435℃



10.稳定性和反应性
Stability and reactivity

稳定性：一般情况下稳定。
Stability: Generally stable.
禁配物: 强酸、强碱。
Incompatible materials: Strong acids and bases.
 
11.毒理学资料
Toxicology Information

急性毒性：无数据资料
Acute toxicity: No data available

12.生态学资料
Ecological information

生态毒性：无数据资料
Ecotoxicity: No data available

13.废弃处置
Waste disposal

废弃处置方法：尽可能回收利用。如果不能回收利用，请采用合适的处置方法。建议掩埋处理，不得采用排放到下水道的方式废弃处置本品。
Waste disposal method: Recycle whenever possible. If recycling is not possible, please use appropriate disposal methods. It is recommended to bury it and dispose of this product by discharging it into the sewer.

14.运输信息
Transport information

运输品名：氧化铬
Transport name: Chromium oxide
危险品分类：普货。
Dangerous goods classification: General goods.
运输注意事项：储存于阴凉、通风仓间内。远离火种、热源。保持容器密封，应与氧化剂、食用化工原料分开存放。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。
Transport precautions: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. Keep the container sealed and store it separately from oxidants and edible chemical raw materials. Load and unload gently during transportation to prevent damage to the packaging and container. Pay attention to personal protection during packaging and transportation.

15.法规信息
Regulatory Information

适用法规：中华人民共和国安全生产法;
中华人民共和国职业病防治法;
中华人民共和国环境保护法;
危险化学品安全管理条例;
安全生产许可证条例。
Applicable regulations: Production Safety Law of the People's Republic of China;
Occupational Disease Prevention and Control Law of the People's Republic of China;
Environmental Protection Law of the People's Republic of China;
Regulations on the Safety Management of Hazardous Chemicals;
Regulations on Production Safety Permits.

16. 其他信息
Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
Modification instructions:Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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