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Safety Data Sheet MSDS
氧化锌
Zinc Oxide 
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：氧化锌
Product Chinese name: Zinc Oxide
产品英文名称：Zinc Oxide
Product English name:  Zinc Oxide
CAS No.：1314-13-2
型号Model：DXN-YC30，DXN-YR30
分子式：ZnO
Molecular formula: ZnO
分子量：81.4084
Molecular weight: 81.4084
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	氧化锌Zinc Oxide
	30%
	应用于抗菌塑料，纺织品，瓷砖，涂料，消毒液等
It is used in antibacterial plastics, textiles, tiles, coatings, disinfectants, etc

	乙醇
Ethanol
	70%
	




3.危险性概述
Hazards Identification

危险性类别：吸入途径：吸入，食入
Hazard Category: Inhalation Route: Inhalation, Ingestion 
健康危害：吸入氧化锌烟尘引起锌铸造热。其症状有口内金属味、口渴、咽干、食欲不振、胸部发紧、干咳、头痛、头晕、四肢酸痛、高热恶寒。大量氧化锌粉尘可阻塞皮脂腺管和引起皮肤丘疹、湿疹。
Health hazards: Inhalation of zinc oxide dust can cause zinc casting fever. Symptoms include metallic taste in the mouth, thirst, dry throat, loss of appetite, chest tightness, dry cough, headache, dizziness, limb pain, high fever and chills. Large amounts of zinc oxide dust can block the sebaceous gland ducts and cause skin papules and eczema.
环境危害：EU分类，对环境有害。
Environmental hazards: EU classification, hazardous to the environment.
燃爆危险：本品可燃。
Explosion hazard: This product is flammable.

4.急救措施
First aid measures
 
皮肤接触：用肥皂水及清水彻底冲洗。就医。
Skin contact: Rinse thoroughly with soap and water. Seek medical attention.
眼睛接触：拉开眼睑，用流动清水冲洗15分钟。就医。
Eye contact: Pull open the eyelids and rinse with running water for 15 minutes. Seek medical attention.
吸入：脱离现场至空气新鲜处。就医。
Inhalation: Leave the scene to a place with fresh air. Seek medical attention.
食入：误服者，口服牛奶、豆浆或蛋清，洗胃。就医。
Ingestion: If ingested by mistake, take milk, soy milk or egg white orally, and wash the stomach. Seek medical attention.

5.消防措施
Fire-fighting measures

危险特性：与镁、亚麻子油发生剧烈反应。与氯化橡胶的混合物加热至215℃以上可能发生爆炸。受高热分解，放出有毒的烟气。
Hazardous characteristics: Reacts violently with magnesium and linseed oil. Mixtures with chlorinated rubber may explode when heated to above 215°C. Decomposes under high heat and emits toxic fumes.
灭火方法及灭火剂：消防人员必须穿全身防火防毒服，在上风向灭火。火场周围可用的灭火介质。
Fire extinguishing methods and extinguishing agents: Firefighters must wear full-body fireproof and anti-gas suits and extinguish fires in the upwind direction. Available extinguishing media around the fire scene.

6.泄露应急处理
Leakage emergency treatment

应急处理：隔离泄漏污染区，周围设警告标志，建议应急处理人员戴好口罩、护目镜，穿工作服。小心扫起，避免扬尘，倒至空旷地方深埋。也可以用大量水冲洗，经稀释的洗水放入废水系统。如大量泄漏，收集回收或无害处理后废弃。
Emergency treatment: Isolate the leaked contaminated area and set up warning signs around it. It is recommended that emergency personnel wear masks, goggles, and work clothes. Sweep it up carefully to avoid dust, and pour it into an open area for deep burial. It can also be rinsed with a large amount of water, and the diluted washing water is put into the wastewater system. In case of large-scale leakage, collect and recycle it or dispose of it harmlessly.

7.操作处置和储存
Handling and storage

操作注意事项：密闭操作，局部排风。操作人员必须经过专门培训，严格遵守操作规程。建议操作人员佩戴自吸过滤式防尘口罩，戴化学安全防护眼镜，穿防毒物渗透工作服，戴乳胶手套。避免产生粉尘。避免与氧化剂接触。搬运时轻装轻卸，防止包装破损。配备泄漏应急处理设备。倒空的容器可能残留有害物。
Operation precautions: Closed operation, local exhaust. Operators must undergo special training and strictly abide by the operating procedures. It is recommended that operators wear self-priming filter dust masks, chemical safety glasses, anti-toxic penetration work clothes, and latex gloves. Avoid generating dust. Avoid contact with oxidants. Load and unload gently during transportation to prevent damage to the packaging. Equipped with leakage emergency treatment equipment. Empty containers may have harmful residues.
储存注意事项：储存于阴凉、通风的库房。远离火种、热源。应与氧化剂分开存放，切忌混储。储区应备有合适的材料收容泄漏物。
Storage precautions: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. It should be stored separately from oxidants and should not be mixed. The storage area should be equipped with suitable materials to contain leaks.

8.接触控制和个体防护
Exposure controls and personal protection

中国 MAC(mg/m3): 5
China MAC (mg/m3): 5
前苏联 MAC (mg/m3) : 5
Former Soviet Union MAC (mg/m3): 5
工程控制：密闭操作，局部排风。
Engineering control: Closed operation, local exhaust.
呼吸系统防护：作业工人建议佩戴防尘口罩。
Respiratory system protection: Workers are recommended to wear dust masks.
眼睛防护：戴化学安全防护眼镜。
Eye protection: Wear chemical safety glasses.
身体防护：防护服。
Body protection: Protective clothing. 
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：及时换洗工作服。注意个人清洁卫生。
Other protection: Change and wash work clothes in time. Pay attention to personal hygiene.

9.理化特性
[bookmark: _GoBack]Physical and chemical properties

	颜色Color
	乳白色Milky

	状态State
	液体Liquid

	气味Odor
	刺激性气味Pungent odor

	相对密度
Relative density
	5.61g/cm3

	PH
	7-9

	熔点Melting point
	-117.3℃

	沸点Boiling point
	78.32℃



10.稳定性和反应性
Stability and reactivity

稳定性：在常温常压下稳定。
Stability: Stable at room temperature and pressure.
有害分解产物：无已知的。
Hazardous decomposition products: None known.
有害聚合：不会发生。
Hazardous polymerization: Will not occur.
禁配物：强氧化剂。
Incompatible materials: Strong oxidants.

11.毒理学资料
Toxicology Information

动物毒数据：LD50>5020.2mg／kg(小鼠经口)
Animal toxicity data: LD50>5020.2 mg/kg (oral in mice)

12.生态学资料
Ecological information

生态有害性：无资料
Ecological harm: No information

13.废弃处置
Waste disposal

废弃处置方法：用安全掩埋法处置。
Waste disposal method: Dispose of in safe landfill.

14.运输信息
Transport information

运输品名：氧化锌
Transport name: Zinc Oxide
危险品分类：普货。
Dangerous goods classification: General goods.
运输注意事项：储存于阴凉、通风仓间内。远离火种、热源。保持容器密封，应与氧化剂、食用化 工原料分开存放。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。
Transport precautions: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. Keep the container sealed and store it separately from oxidants and edible chemical raw materials. Load and unload gently during transportation to prevent damage to the packaging and container. Pay attention to personal protection during packaging and transportation.

15.法规信息
Regulatory Information

适用法规：化学危险物品安全管理条例 (1987年2月17日国务院发布)，化学危险物品安全管理条例实施细则 (化劳发[1992] 677号)，工作场所安全使用化学品规定 ([1996]劳部发423号)等法规，针对化学危险品的安全使用、生产、储存、运输、装卸等方面均作了相应规定。
Applicable regulations: Regulations on the Safety Management of Hazardous Chemicals (issued by the State Council on February 17, 1987), Rules for the Implementation of the Regulations on the Safety Management of Hazardous Chemicals (Chemical Labor Department [1992] No. 677), Regulations on the Safe Use of Chemicals in the Workplace (Labor Department [1996] No. 423), and other regulations have made corresponding provisions for the safe use, production, storage, transportation, loading and unloading of hazardous chemicals.

16.其他信息
Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
Modification instructions：Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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