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Safety Data Sheet MSDS
氧化锡
Stannic Oxide 
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：氧化锡Product Chinese name: Stannic Oxide
产品英文名称：Stannic Oxide
Product English name:  Stannic Oxide
CAS No.：18282-10-5
型号Model：DXN-SY30.
分子式：SnO2
Molecular formula: SnO2
分子量：150.69
Molecular weight: 150.69
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	氧化锡Stannic Oxide
	30%
	制造半导体电子工业材料、陶瓷釉料、气敏元件材料、搪瓷和电磁材料等
Manufacture of semiconductor electronic industry materials, ceramic glazes, gas-sensitive component materials, enamel and electromagnetic materials, etc

	乙醇
Ethanol
	70%
	




3.危险性概述
Hazards Identification

危险类别（GHS）：非危险物质或混合物。
Hazard Class (GHS): Not a hazardous substance or mixture.

4.急救措施
First aid measures
 
皮肤接触：将受污染的衣物和鞋子移除，用水和肥皂清洗患处 15 分钟以上。若有需要，立即就医。
Skin contact: Remove contaminated clothing and shoes and wash the affected area with water and soap for at least 15 minutes. Seek medical attention if necessary.眼睛接触：拉开眼睑，用流动清水冲洗15分钟。就医。
Eye contact: Pull open the eyelids and rinse with running water for 15 minutes. Seek medical attention.
吸入：如果吸入,请将患者移到新鲜空气处。如果停止了呼吸,给于人工呼吸。 
Inhalation: If inhaled, move victim to fresh air. If not breathing, give artificial respiration.
食入：切勿给失去知觉者从嘴里喂食任何东西。用水漱口。
Ingestion: Never give anything by mouth to an unconscious person. Rinse mouth with water.

5.消防措施
Fire-fighting measures

灭火方法及灭火剂：本品可燃。尽可能将容器从火场移至空旷处。
Fire extinguishing methods and extinguishing agents: This product is flammable. Move containers from the fire to an open area as much as possible. 
源于此物质或混合物的特别的危害：如必要的话,戴自给式呼吸器去救火。
Special Hazards: If necessary, wear self-contained breathing apparatus for firefighting.

6.泄露应急处理
Leakage emergency treatment

人员的预防,防护设备和紧急处理程序：防止粉尘的生成，避免吸入粉尘。撤出危险区域，遵守紧急措施，请教专业人员，防止吸入蒸汽、气雾或气体。
Personal precautions, protective equipment and emergency procedures: Prevent dust formation and avoid inhalation of dust. Evacuate the danger zone, follow emergency procedures, consult a qualified professional, and avoid inhalation of vapors, mists or gases.
环境预防措施:不要让产物进入下水道。
Environmental precautions: Do not allow product to enter drains.
抑制和清除溢出物的方法和材料: 遵照可能的物质使用限制。干燥处理，并依化学废弃物处置，清理受影响的区域。避免生成粉尘。
Methods and materials for containment and cleanup: Observe possible restrictions on the use of substances. Handle dry and dispose of as chemical waste and clean up affected area. Avoid the creation of dust.

7.操作处置和储存
Handling and storage

安全操作的注意事项:在有粉尘生成的地方,提供合适的排风设备。避免吸入物质/混合物。
Precautions for safe handling: Provide suitable exhaust equipment where dust is generated.Avoid inhalation of substance/mixture.
安全储存的条件,包括任何不兼容性:储存于阴凉、通风的库房。远离火种、热源。应与酸类，碱分开存放放，切忌混储。储区应备有合适的材料收容泄漏物。
Conditions for safe storage, including any incompatibilities: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. Store separately from acids and alkalis and avoid mixing. The storage area should be equipped with appropriate materials to contain leaks.

8.接触控制和个体防护
Exposure controls and personal protection

工程控制：尽可能安装封闭体系或局部排风系统，操作人员切勿直接接触。同时安装淋浴器和洗眼器。
Engineering control:Install a closed system or local exhaust system as much as possible, and operators should not come into direct contact with it. Also install a shower and eyewash station.
呼吸系统防护：作业工人建议佩戴防尘口罩。
Respiratory system protection: Workers are recommended to wear dust masks.
眼睛防护：戴化学安全防护眼镜。
Eye protection: Wear chemical safety glasses.
身体防护：防护服。
Body protection: Protective clothing. 
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：及时换洗工作服。注意个人清洁卫生。
Other protection: Change and wash work clothes in time. Pay attention to personal hygiene.

9.理化特性
Physical and chemical properties

	颜色Color
	浅灰色Light gray

	状态State
	液体Liquid

	气味Odor
	刺激性气味Pungent odor

	溶解度
Solubility
	不溶于水，溶于浓硫酸、盐酸
Insoluble in water, soluble in concentrated sulfuric acid and hydrochloric acid

	[bookmark: _GoBack]沸点Boiling point
	78.32℃

	熔点Melting point
	-117.3℃



10.稳定性和反应性
Stability and reactivity

稳定性：本产品在标准大气状态(室温)下化学性质稳定。
Stability: The chemical properties of this product are stable under standard atmospheric conditions (room temperature).
应避免的物质: 强氧化剂, 强酸和强碱, 强还原剂, 碱金属。
Substances to avoid: Strong oxidizing agents, Strong acids and bases, Strong reducing agents, Alkali metals.

11.毒理学资料
Toxicology Information

急性毒性：LD50 吞食 - 大鼠 - > 20,000 mg/kg
LC50 吸入 - 大鼠 - 雄性和雌性 - 4 h - > 2.04 mg/l - 粉尘／烟尘
Acute toxicity: LD50 ingestion - rat - > 20,000 mg/kg
LC50 inhalation - rat - male and female - 4 h - > 2.04 mg/l - dust/fume

12.生态学资料
Ecological information

无资料No data

13.废弃处置
Waste disposal

废弃处置方法：化学品必需依废弃物清理法清理。产品必需按照国家法规的规定丢弃或导入设计好的回收系统。 废料的排放必须符合国家及当地法规的规范。废弃化学品请保留于原容器中，勿与其他废弃物混和。依照处理产品的相同标准处理不洁的容器。
Waste disposal method: Chemicals must be disposed of in accordance with waste disposal laws. Products must be discarded or directed to a designed recycling system in accordance with national regulations. Waste discharge must comply with national and local regulations. Keep waste chemicals in their original containers and do not mix with other waste. Dispose of unclean containers in the same manner as products.

14.运输信息
Transport information

运输品名：氧化锡
Transport name: Stannic Oxide
危险品分类：普货。
Dangerous goods classification: General goods.
运输注意事项：储存于阴凉、通风仓间内。远离火种、热源。保持容器密封，应与氧化剂、食用化工原料分开存放。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。
Transport precautions: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. Keep the container sealed and store it separately from oxidants and edible chemical raw materials. Load and unload gently during transportation to prevent damage to the packaging and container. Pay attention to personal protection during packaging and transportation.

15.法规信息
Regulatory Information

适用法规：中华人民共和国安全生产法;
中华人民共和国职业病防治法;
中华人民共和国环境保护法;
危险化学品安全管理条例;
安全生产许可证条例。
Applicable regulations: Production Safety Law of the People's Republic of China;
Occupational Disease Prevention and Control Law of the People's Republic of China;
Environmental Protection Law of the People's Republic of China;
Regulations on the Safety Management of Hazardous Chemicals;
Regulations on Production Safety Permits.

16. 其他信息
Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
Modification instructions：Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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