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Safety Data Sheet MSDS
氧化镧
Lanthanum Oxide 
                              编号:DXN2024MSDS
                                                       初始版：DXN2018.11.1版
                                                       修订日期：2024年8月1日
1. 产品名称和制造商信息
Product name and manufacturer information
产品中文名称：氧化镧Product Chinese name: Lanthanum Oxide
产品英文名称：Lanthanum Oxide
Product English name:  Lanthanum Oxide
CAS No.：1312-81-8 
型号Model：DXN-LA100/DXN-LA120
分子式：La2O3
Molecular formula: La2O3
分子量：325.84
Molecular weight: 325.84
供应商：达西浓纳米科技（常州）有限公司
Supplier: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
生产厂商：山东科纳达新材料科技有限公司
Manufacturer: Shandong Konada New Material Technology Co., Ltd.
地址：常州市新北区辽河路901号新科创大楼A座第四层410号
Address: Room 410, 4th Floor, Building A, New Science and Technology Innovation Building, No. 901 Liaohe Road, Xinbei District, Changzhou
电话/传真：+86-0519-85558068
Tel/Fax: +86-0519-85558068
紧急联系电话：+86-0519-85558068
Emergency contact number: +86-0519-85558068

2.成分/组成信息
Composition/ingredient information

  描述：物质成分配比
Description: Material composition ratio
	物质成分名称
Name of material component
	比重（%）
proportion(%)
	用途
Use

	氧化镧
Lanthanum Oxide
	[bookmark: _GoBack]99.999%
	用于制造精密光学玻璃、光导纤维。也用于电子工业作陶瓷电容器，压电陶瓷掺入剂等
Used to manufacture precision optical glass and optical fibers. Also used in the electronics industry to make ceramic capacitors, piezoelectric ceramic doping agents, etc.




3.危险性概述
Hazards Identification

危险类别（GHS）：非危险物质或混合物。
Hazard Class (GHS): Not a hazardous substance or mixture.

4.急救措施
First aid measures
 
皮肤接触：脱去污染的衣着，用肥皂水和清水彻底冲洗皮肤。如有不适感，就医。
Skin contact: Remove contaminated clothing and rinse skin thoroughly with soap and water. Seek medical attention if you feel unwell.
眼睛接触：分开眼睑，用流动清水或生理盐水冲洗。立即就医。
Eye contact: Open the eyelids and rinse with running water or saline. Seek medical attention immediately.
吸入：如果吸入，请将患者移到新鲜空气处。
Inhalation: If inhaled, move victim to fresh air.
食入：: 请清洗口腔。不要引发呕吐。
Ingestion: Rinse mouth. Do not induce vomiting.

5.消防措施
Fire-fighting measures

灭火方法及灭火剂：用水雾,抗乙醇泡沫,干粉或二氧化碳灭火。避免使用直流水灭火，直流水可能导致可燃性液体的飞溅，使火势扩散。
Fire extinguishing methods and extinguishing agents: Use water spray, alcohol-resistant foam, dry powder or carbon dioxide to extinguish fire.Avoid using direct water to extinguish fire, as direct water may cause flammable liquids to splash and spread the fire.
特殊情况:在加热期间或失火的情况下,产生有毒气体。
Special cases: During heating or in case of fire, toxic gases are generated.

6.泄露应急处理
Leakage emergency treatment

人员的预防,防护设备和紧急处理程序：建议应急处理人员戴携气式呼吸器，穿防静电服，戴橡胶耐油手套。禁止接触或跨越泄漏物。作业时使用的所有设备应接地。尽可能切断泄漏源。消除所有点火源。根据液体流动、蒸汽或粉尘扩散的影响区域划定警戒区，无关人员从侧风、上风向撤离至安全区。
Personal precautions, protective equipment and emergency procedures: It is recommended that emergency response personnel wear air-carrying respirators, anti-static clothing, and rubber oil-resistant gloves. It is prohibited to touch or cross the leaked material. All equipment used during operation should be grounded. Cut off the source of leakage as much as possible. Eliminate all ignition sources. Delineate warning areas according to the affected areas of liquid flow, steam or dust diffusion, and evacuate irrelevant personnel from the sidewind and upwind directions to safe areas.
环境预防措施:用大量的水进行稀释。切勿让其进入下水道/水面或地下水。
Environmental precautions: Dilute with plenty of water. Do not allow to enter drains/surface or ground water.
抑制和清除溢出物的方法和材料:扫掉和铲掉。 存放在合适的封闭的处理容器内。
Methods and materials for containment and cleanup: Sweep up and shovel. Store in suitable closed disposal containers.

7.操作处置和储存
Handling and storage

安全操作的注意事项:在有粉尘生成的地方,提供合适的排风设备。
Precautions for safe handling: Provide suitable exhaust equipment where dust is generated.
安全储存的条件,包括任何不兼容性:贮存在阴凉处.容器保持紧闭，储存在干燥通风处。防止气溶胶的形成。
Conditions for safe storage, including any incompatibilities: Store in a cool place. Keep the container tightly closed in a dry and ventilated place.Prevent the formation of aerosols.

8.接触控制和个体防护
Exposure controls and personal protection

控制参数:最高容许浓度没有已知的国家规定的暴露极限。
Control parameters: Maximum permitted concentration There are no known national exposure limits.
工程控制：常规的工业卫生操作。
Engineering control:General industrial hygiene practices.
呼吸系统防护：作业工人建议佩戴防尘口罩。
Respiratory system protection: Workers are recommended to wear dust masks.
眼睛防护：戴化学安全防护眼镜。
Eye protection: Wear chemical safety glasses.
身体防护：防护服。
Body protection: Protective clothing. 
手防护：配戴防护手套。
Hand protection: Wear protective gloves.
其他防护：及时换洗工作服。注意个人清洁卫生。
Other protection: Change and wash work clothes in time. Pay attention to personal hygiene.

9.理化特性
Physical and chemical properties

	颜色Color
	白色White

	状态State
	粉末Powder

	气味Odor
	无味Odorless

	溶解度
Solubility
	可溶于无机酸生成盐，不溶于水
Soluble in inorganic acid to form salt, insoluble in water

	相对密度
Relative density
	6.51

	熔点Melting point
	>2000℃



10.稳定性和反应性
Stability and reactivity

应避免的条件：避免潮湿
Conditions to avoid: Avoid moisture
禁配物:强酸, 强氧化剂, 二氧化碳 (CO2)
Incompatible materials: Strong acids, Strong oxidants, Carbon dioxide (CO2)
危险的分解产物: 在加热期间或失火的情况下,可能会形成有毒的气体。
Hazardous Decomposition Products: During heating or in the event of fire, toxic gases may be formed.
 
11.毒理学资料
Toxicology Information

急性毒性：经口: LD50 - rat (male/female) - > 10 000 mg/kg bw 
吸入: LC0 - rat (male/female) - >= 5.3 mg/L air (analytical) 
经皮: LD50 - rabbit - > 2 000 mg/kg bw
潜在影响：吸入摄入会引起呼吸道刺激。
Potential Effects: Inhalation may cause respiratory irritation.

12.生态学资料
Ecological information

生态毒性：对水蚤和其他水生无脊固定 无可观察效应浓度 - 大型蚤 (水蚤) - >= 100 mg/l - 48 h
椎动物的毒性方法: 经济合作和发展组织的试验指导书202
Ecotoxicity: Toxicity to daphnia and other aquatic invertebrates No observable effect concentration - Daphnia magna (Water flea) - >= 100 mg/l - 48 h
Toxicity to vertebrates Method: OECD Test Guideline 202

13.废弃处置
Waste disposal

废弃处置方法：尽可能回收利用。如果不能回收利用，采用焚烧方法进行处置。不得采用排放到下水道的方式废弃处置本品。
Waste disposal method: Recycle as much as possible. If recycling is not possible, dispose of it by incineration. Do not dispose of this product by discharge into the sewer.

14.运输信息
Transport information

运输品名：氧化镧
Transport name: Lanthanum Oxide
危险品分类：普货。
Dangerous goods classification: General goods.
运输注意事项：储存于阴凉、通风仓间内。远离火种、热源。保持容器密封，应与氧化剂、食用化工原料分开存放。搬运时要轻装轻卸，防止包装及容器损坏。分装和搬运作业要注意个人防护。
Transport precautions: Store in a cool, ventilated warehouse. Keep away from fire and heat sources. Keep the container sealed and store it separately from oxidants and edible chemical raw materials. Load and unload gently during transportation to prevent damage to the packaging and container. Pay attention to personal protection during packaging and transportation.

15.法规信息
Regulatory Information

适用法规：中华人民共和国安全生产法;
中华人民共和国职业病防治法;
中华人民共和国环境保护法;
危险化学品安全管理条例;
安全生产许可证条例。
Applicable regulations: Production Safety Law of the People's Republic of China;
Occupational Disease Prevention and Control Law of the People's Republic of China;
Environmental Protection Law of the People's Republic of China;
Regulations on the Safety Management of Hazardous Chemicals;
Regulations on Production Safety Permits.

16. 其他信息
Other information

制表单位：达西浓纳米科技（常州）有限公司
Tabulation units: DASHINOU NANO TECHNOLOGY（CHANG ZHOU）CO.，LTD.
联系电话：+86-0519-85558068
Contact number：+86-0519-85558068
修改说明：根据我们所掌握的最新信息进行编写，所提供的信息仅为安全操作、使用、加工、储存、运输、处置和排放的参考，不能作为相关保证。表中信息仅用于指定特定的物质，不适用于结合了其他任何物质或经过加工的物质。使用者应根据使用目的，对相关信息的合理性做出判断。
Modification instructions：Prepared based on the latest information available to us, the information provided is only a reference for safe operation, use, processing, storage, transportation, disposal and discharge and cannot be used as a guarantee. The information in the table is intended only to specify the specific substance and does not apply to substances combined with any other substances or processed. Users should make judgments on the rationality of relevant information based on the purpose of use.
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